Running results:

Structure of meta-surface：

when Width=70nm,Length=201nm,Height=330nm, Phi=90

the efficiency of T\_RCP=86.65%，while T\_LCP =2.91%